|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ESTD : 1996**  **Lakshmi&Co**  **GSTIN: 33ACXPN0903A1ZY** | | | | | | | | | |
| **Address:**  **30,Amman Kovil Street, Venkitapuram,**  **G.C.T.Post, Coimbatore-641013.Tamilnadu.INDIA**  **Email:** [**brickmachineries.in@gmail.com**](mailto:brickmachineries.in@gmail.com)  **Websites:**[**www.brickmachineries.in**](http://www.brickmachineries.in) [**www.claybrick.in**](http://www.claybrick.in)[**www.ashbrick.in**](http://www.ashbrick.in) | | | | **Mobile No:+91-9944936701 / 703 / 705**  **Whatsapp:+91-9944936702 / 704**  **Landline:+91422-2437208 / 2436129** | | | | | |
| **To** | | | | | **Quotation/Estimation** | | | | |
| **Date:** |  | | | |
| **REF No:** |  | | | |
| **Customer Email:** | | **GST:** | | | **Contact:** | | | | |
| **S.No** | **Particulars** | | **HS. Code** | | **Rate**  **INRs** | | **Qty** | **Amount**  **INRs Ps** | |
| **1**    **2**  **3**  **4**  **5** | **Model-WC-4000**  Wire cut double Shaft Extruder: Pug Mill Wire cut brick making Machine (2500 to 3500 Brick Per Hour approx ) Two Rollers Power40 Hp or 50 Hp Motor Or Diesel Engine ( Clay Crushing and Extrusion in Brick Form ) With Motor and one Brick Mouth SS shim 250 mm X 120 mm or customer size With Brick Sizes :  1, **L 9” X W 6” X H 3”** = 2. **L 9” X W 4” X H 3”** = 3. **L 9” X W 6” X H 3”**  4. **L 9” X W 4” X H 2 ¼ ”**  = 5. **L 8” X W 3 ½ ” X H 2 ¼ ”**  **Box Feeder**  **Clay Mixing Machine Power 15 Hp 1440 RPM**  **Clay Grinding Rollers Units Power 10 Hp 960 Rpm**  **Brick Cutting Table 10 Brick in One Stroke Hydraulic Operated**  **Extra Fitting :Belt Conveyor 20’ Feet Length Power**    **(Total-Indian Rupees Thirty two lakhs twentyone thousand and four hundred Only)** | | **8474 80 10**  **xxxx xx xx** | | **15,00,000**  **4,75,000**  **2,50,000**  **1,65,000**  **1,70,000** | | **1**  **1**  **1**  **1**    **2** | **15,00,000**  **4,75,000**  **2,50,000**  **1,65,000**  **3,40,000** | **00**  **00**  **00**  **00**    **00** |
| **\*Terms&Conditions**  **\*ERECTION CHARGES: RS:1000 Per day,**  **\*LOADING: By Lakshmi&co @Free of cost \*UNLOADING: By Party. \*FREIGHT: By Party actual.**  **\*DELIVERY: 40 days, \*ADVANCE 40%, BALANCE: 60% AT EX-FACTORY COIMBATORE. \*VALIDITY: 90 DAYS, \*WARRANTY: 12MONTHS.\*Insurance 1% By Party**  **\*Discount applicable only on confirmation.(Optional) \*valid for Tamilnadu only**  **Subject to Coimbatore Jurisdiction** | | | | | **Total:**  **CGST 9 %**  **SGST 9 %**  **Grand Total** | | | **27,30,000**  **2,45,700**  **2,45,700** | **00**  **00**  **00** |
| **32,21,400** | **00** |
|  |  |
|  |  |

**For Lakshmi&co**

**Authorized Signatory**

Box Feeder Clay Crusher Extruder/ Pugmill Hydro Wirecut Table

   